Id
Talkgroup identifier in decimal format.

Id is already defined Id is invalid Id is required

Label
Talkgroup label displayed on the main screen and on buttons.

Label is required

Name
Talkgroup name displayed on the main screen.

Name is required

Groups
Groups to which this talkgroups belongs.

{{ group.label }} Group is required

Tag
Tag to which this talkgroups belongs.

{{ tag.label }} Tag is required

Audio alert
Prefixes an alert sound to all calls assigned from this talkgroup. The alert assignment order is as follows: Group -> Tag -> System -> Talkgroup.

No Alert {{ alert | titlecase }}

Delay
Delay in minutes before propagating calls to clients.

Frequency
Fake frequency in hertz displayed on the main screen.

Invalid frequency

Led Color
The default LED color is green but it can be changed at several levels. The color assignment order is as follows: Group -> Tag -> System -> Talkgroup.

Default {{ led | titlecase }}

Type
Type of radio system that will override the type defined at the system level, if any.

- AM - Amplitude modulation.
- DMR - Digital mobile radio system.
- FM - Frequency modulation.
- NFM - Narrow frequency modulation.
- NXDN - Next Generation Digital Narrowband radio system.
- P25 - APCO-25 radio system.
- Provoice - EDACS Provoice radio system.
- SmartNet - Motorola SmartNet radio system.
- Tetra - Trans european trunked radio system.

No Type AM DMR FM NFM NXDN P25 Provoice SmartNet Tetra