# Touchscreen Keypads
## Models
KXPi-100W - White
KXPi-100B - Black
KXPi-100G - Grey
KXPi-100WG - Wood Grain

## Installation
1. Create a folder in your security system, name it whatever (We use TouchScreens, but it can be anything)
2. Place the KXPi-100 inside this folder
3. Upload voice_mega.ogg via Asset Manager and set the asset id inside the keypad Audio part. (Required for any voice/tones)
4. Connect the API2 ObjectValue to API2 in your security system.
5. It should work!